**FULLY REUSED VLSI ARCHITECTURE OF FM0/MANCHESTER ENCODING USING SOLS TECHNIQUE FOR DSRC APPLICATIONS**

**Abstract:**

 The dedicated short-range communication (DSRC) is an emerging technique to push the intelligent transportation system into our daily life. The DSRC standards generally adopt FM0 and Manchester codes to reach dc-balance, enhancing the signal reliability. Nevertheless, the coding-diversity between the FM0 and Manchester codes seriously limits the potential to design a fully reused VLSI architecture for both. In this paper, the similarity-oriented logic simpliﬁcation (SOLS) technique is proposed to overcome this limitation. The SOLS technique improves the hardware utilization rate from 57.14% to 100% for both FM0 and Manchester encodings. The performance of this paper is evaluated on the postlayout simulation in Taiwan Semiconductor Manufacturing Company (TSMC) 0.18-µm 1P6M CMOS technology. The maximum operation frequency is 2 GHz and 900 MHz for Manchester and FM0 encodings, respectively. The power consumption is 1.58 mW at 2 GHz for Manchester encoding and 1.14 mW at 900 MHz for FM0 encoding. The core circuit area is 65.98 × 30.43 µm2. The encoding capability of this paper can fully support the DSRC standards of America, Europe, and Japan. This paper not only develops a fully reused VLSI architecture, but also exhibits an efﬁcient performance compared with the existing works.

**Index Terms—**Dedicated short-range communication (DSRC), FM0, Manchester, VLSI.

**TOOLS:**

1. **XilinxISE 14.7**

**LANGUAGE:**

1. **VerilogHDL**